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Date: 16th July 2026
INVITATION TO BIDS
Pakistan Poverty Alleviation Fund (PPAF) invites sealed bids from eligible bidders for procurement of Equipment/Machinery.

Bids must be delivered to the below-mentioned office address on or before 11:00 AM on 31st July 2026 and must be accompanied by a bid security of 2% of the total bid amount in form of Bank Draft/Pay order and a bid fee of Rs. 5000/-. The bids will be opened on the same date i.e 31st July 2026 at 11:30 AM in the presence of bidders. 

Interested eligible bidders may download the bidding document by clicking on the weblink i.e. https://www.ppaf.org.pk/goods

Procurement Section

Pakistan Poverty Alleviation Fund (PPAF)

Plot 14, Street 12, Mauve Area, G-8/1, Islamabad.

UAN: (92-51) 111-000-102; Ph: (051) 8439450-79

Fax: (92-51) 2282262 & 4, Website: www.ppaf.org.pk

INSTRUCTION TO BIDDERS

Date: 16th July 2026
1. Single stage two envelopes method shall be adopted for this procurement. The selection will be based on quality and cost.
2. The Bid must be enclosed in one sealed envelope with name and return address of bidder submitting the Bid.
3. Any firm / group of firms found involved in creating a cartel or any other collusion arrangement against the interest of the organization, will be blacklisted and debarred.

4. The bidder shall specify bid validity in days. PPAF may request the bidder for extension in bid validity, if required.

5. In case of difference between bid amount (amount in numbers and amount in words), the amount in words will prevail. Overwriting in the Bid is strictly prohibited.

6. Bid Submission: Sealed bids should reach our Office “Plot # 14, Street 12, Mauve Area, G-8/1, Islamabad on or before 31st July 2026, at 11:00 AM. 

7. Bid Fee: The interested bidders shall attach a Demand Draft/Pay Order (non-refundable) of Rs. 5,000/- (rupees five thousand only) along with their Technical Bid otherwise the bid will be rejected. 

8. Opening of Bids: Bids will be opened on the same day i.e., 31st July 2026, at 11:30 AM in presence of the bidders’ representatives who chose to participate.
9. In case a public holiday is announced by the Government (Due to any reason) the Bids will be opened the next working day at the same time and venue.

10. Bid Security: 2% of the total bid amount, in shape of Bank Draft/Pay order in favor of “Pakistan Poverty Alleviation Fund” must be attached with the bid as Bid Security. Bids received without Bid Security shall be rejected.  

11. Delivery Time: Within 4-8 weeks after signing the Purchase Order.
12. Bid Validity: Bids shall be valid for a period of 45 days.

13. Bid Currency: Currency shall be Pakistani Rupees (PKR).

14. Bid Price: The prices must be inclusive of all taxes, duties, delivery / transportation and other allied costs to the final destination. 
15. The quantity of the item(s) may increase or decrease. Besides, one or more items could be eliminated. 
16. Lower specifications will lead to disqualification. 
17. Incomplete or late received offers will not be considered.
18. Cancellation of the bidding procedure: PPAF reserves the right to cancel/reject any or all offers, and/or cancel the entire bidding process at any stage without assigning any reason (s) thereof.
SELECTION CRITERIA

All bids shall be evaluated under single stage two envelopes procedure (Technical Bid and Financial Bid in a single sealed envelope).
TECHNICAL QUALIFICATION CRITERIA

The bidders must fulfil the following mandatory criteria, those bidders who don’t fulfil the criteria shall be rejected (even a single missing document shall lead to disqualification). The contract shall be awarded to the lowest eligible bidder as per required specification. 

	Mandatory documents (Stage-1 evaluation)
	Score

	Technical Criteria

	1. 
	GST registration Certificate. NTN Certificate (with proof of being active).
	GST= 5 marks

Active Taxpayer= 5 marks

	2. 
	Total experience of the firm/bidder (Purchase orders/contracts copies of past 03 years)
	30 marks

	
	Affidavit on a stamp paper stating that the bidder has never been blacklisted by any government/semi-government and non-government organization 
	10 marks

	
	Turnover of last one year 

Proof of bank account in the name of business along with last one year bank statement.
	Maximum 20 marks

(Above 50 M= 20 marks

30-50 M= 15 marks

Below 30 M= 10 marks)

	(Stage-2 evaluation)
	Score

	Financial Criteria

	3. 
	Financial Bid
	30 marks

Financial score= Lowest bid/bid under consideration x 30


Note: Minimum of 50 marks in Technical Criteria (S. No. 1 to 4) are required to qualify for Stage-2 evaluation process. 
Pre Bid Meeting: For clarifications (if any), a pre bid meeting will be held on 23rd July 2026 from 11:30 a.m. to 12:00 p.m. The interested bidders may choose to attend the meeting via link (Microsoft Teams) given below:

Microsoft Teams meeting 

Join: https://teams.microsoft.com/meet/42099312889410?p=Geire93ykwNeOToJc6 

Meeting ID: 420 993 128 894 10 

Passcode: LR34gb2r 

DETAIL OF LOT AND QUANTITY

Please submit the bids (Unit price in Pak Rs. inclusive of all taxes and allied expenses at the final destination(s).
Lot 01- Equipment/Machinery for Peanut Processing Unit
	S. NO


	Description

	Qty


	Unit Price in PKR including applicable taxes 
	Total Price in PKR including applicable taxes

	Laptops

	1
	Processor
Intel Core Ultra 7 or equivalent, latest/current generation at the time of bidding; minimum 8 cores.
Memory
Minimum 16 GB DDR5/LPDDR5x RAM.
Storage
Minimum 512 GB PCIe NVMe SSD.
Display
14-inch, minimum 1920 × 1200 (WUXGA) or FHD equivalent, anti-glare.
Graphics
Integrated graphics suitable for enterprise productivity and multimedia.
Camera
Integrated FHD 1080p webcam with privacy shutter.
Audio
Integrated speakers and microphone.
Wireless
Minimum Wi-Fi 6E and Bluetooth 5.3 or higher.
Ports
Minimum 2 × USB-A, 1 × USB-C with charging/display capability, and HDMI. Additional USB-C/Thunderbolt/USB4 acceptable.
Keyboard
Standard notebook keyboard; backlit preferred.
Security
TPM 2.0, Secure Boot, BIOS/UEFI password support; fingerprint reader or IR camera preferred.
Battery
Minimum 50 Wh or OEM-rated battery suitable for normal business use.
Power Adapter
OEM-supplied compatible AC/USB-C power adapter.
Operating System
Genuine Windows 11 Pro 64-bit, OEM pre-installed and activated.
Weight
Preferably 1.6 kg or less.
Build
Business/enterprise-class chassis designed for professional use.
Warranty
Minimum 3-year OEM warranty, preferably on-site.
Condition
Brand new, unused, current production model; not refurbished or discontinued.
Accessories
OEM power adapter and standard carrying bag.

	5
	
	

	Noise-Cancelling Headsets

	2
	Parameter
Minimum Required Specification
Type
Professional/business-grade wireless headset.
Wearing Style
Over-the-head, binaural (dual-ear).
Connectivity
Bluetooth wireless connectivity.
Computer Connectivity
Dedicated USB-A and/or USB-C Bluetooth adapter/dongle.
Active Noise Cancellation
Built-in Active Noise Cancellation (ANC).
Microphone
Integrated boom microphone with advanced background noise reduction/noise cancellation.
Audio
Wideband audio with clear voice and multimedia support.
Wireless Range
Minimum 30 metres in open environment.
Talk Time
Minimum 20 hours per charge.
Charging
USB charging; USB-C preferred.
Multi-Device
Ability to connect to at least two devices simultaneously.
Controls
Call answer/end, mute/unmute and volume controls.
Mute Function
Dedicated mute control with visual and/or audible indication.
Compatibility
Compatible with Windows 11 and major unified communication platforms.
UC Support
Certified or optimized for Microsoft Teams or equivalent enterprise collaboration platform.
Comfort
Adjustable headband and cushioned ear pads suitable for extended office use.
Accessories
USB wireless adapter/dongle, charging cable and carrying pouch/case.
Warranty
Minimum 2-year OEM warranty.
Condition
Brand new, unused and current production model.

	5
	
	

	24-Port Managed Network Switch

	3
	Parameter
Minimum Required Specification
Switch Type
Enterprise-grade, fully managed Layer 2+ / Layer 3 access switch.
Access Ports
Minimum 24 × 10/100/1000 Mbps Gigabit Ethernet RJ-45 ports.
Uplink Ports
Minimum 4 × 1/10 Gigabit SFP/SFP+ uplink ports.
PoE
PoE Enabled.
Switching Capacity
Minimum 90 Gbps.
Forwarding Rate
Minimum 65 Mpps.
MAC Address Table
Minimum 16,000 MAC addresses.
VLAN Support
IEEE 802.1Q; minimum 1,000 active VLANs.
Layer 2 Features
VLAN, 802.1Q, STP, RSTP, MSTP, LACP/EtherChannel or equivalent, LLDP and port mirroring.
Layer 3 Features
IPv4/IPv6 static routing and inter-VLAN routing.
Security
IEEE 802.1X, port security, ACLs, DHCP Snooping, Dynamic ARP Inspection and IP Source Guard.
Authentication
RADIUS and TACACS+ or equivalent centralized AAA support.
QoS
Enterprise QoS with traffic classification, marking, prioritization and multiple queues.
Management
CLI, SSH, HTTPS/Web management, SNMP v2c/v3, Syslog and NTP.
Stacking
Hardware or virtual stacking capability preferred.
IPv6
IPv6 management and security support.
Form Factor
Standard 1U, 19-inch rack mountable.
Power
220–240V AC, 50Hz compatible.
Accessories
Rack-mounting kit, power cord and necessary standard accessories.
Warranty
Minimum 3-year OEM warranty/support.
Product Status
Brand new, unused, current production model and not declared End-of-Sale or End-of-Support at bid submission.

	01
	
	

	UPS System

	4
	Parameter
Minimum Required Specification
UPS Type
True Online, Double-Conversion UPS.
Rated Capacity
Minimum 5 kVA.
Output Power
Minimum 4.5 kW; 5 kW preferred.
Input
Single-phase AC, compatible with 220–240V, 50Hz.
Output
Single-phase AC, 220/230/240V selectable, 50Hz.
Output Power Factor
Minimum 0.9; unity (1.0) preferred.
Input Power Factor
Minimum 0.99 at full load.
Output Waveform
Pure sine wave.
Technology
Online double conversion with zero transfer time to battery mode.
Transfer Time
0 ms in normal online-to-battery operation.
Efficiency
Minimum 94% in online mode; high-efficiency/ECO mode preferred.
Voltage Regulation
Output voltage regulation ±1% or better.
Overload Protection
Built-in overload protection with automatic bypass.
Bypass
Automatic/static bypass; manual maintenance bypass preferred.
Battery Type
Maintenance-free sealed lead-acid (VRLA) batteries or equivalent.
Backup Time
Minimum 15 minutes at 50% load, or as specified by the purchaser.
Battery Management
Intelligent battery charging and battery health monitoring.
Cold Start
Supported.
Display
LCD showing input/output voltage, load, battery status, alarms and operating mode.
Communication
USB and/or RS-232 interface.
Network Management
SNMP/network management capability; SNMP card included where remote monitoring is required.
Protection
Overload, short circuit, over/under-voltage, battery discharge and surge protection.
Alarms
Audible and visual alarms for battery mode, low battery, overload and faults.
Form Factor
Tower or rack/tower convertible, as required.
Installation
Supply, installation, testing and commissioning included.
Warranty
Minimum 2-year comprehensive warranty for UPS and batteries.
Condition
Brand new, unused and current production model.

	01
	
	

	Data Backup & Recording System

	5
	LED Display

CRM/Call Center Software
	01

01
	
	

	SIP/Hosted PBX Setup/IP Phones

	6
	Parameter
Minimum Required Specification
Type
Enterprise-grade, desk-based IP Phone.
VoIP Protocol
SIP-based IP telephony; compatible with the organization's existing IP telephony infrastructure.
Line Keys
Minimum 4 programmable line/feature keys.
Display
Minimum 3.5-inch graphical display; color display preferred.
Network Ports
Minimum 2 × 10/100/1000 Mbps Gigabit Ethernet ports with integrated Ethernet switch.
PoE
IEEE 802.3af PoE support.
External Power
Support for external AC power adapter, if required.
Audio
HD/Wideband audio.
Speakerphone
Full-duplex hands-free speakerphone.
Headset Support
Dedicated headset connectivity; RJ-9, USB, Bluetooth or equivalent.
Codec Support
G.711, G.722 and other standard enterprise voice codecs.
Call Features
Hold, transfer, conference, call forward, redial, mute, voicemail access, call history and directory.
Security
Secure provisioning and encrypted signaling/media where supported by the existing IP telephony system.
VLAN / QoS
IEEE 802.1Q VLAN and IEEE 802.1p/Q or equivalent voice traffic prioritization.
Network Services
DHCP, DNS, NTP and LLDP/LLDP-MED support.
Management
Centralized provisioning and remote configuration capability.
Compatibility
Fully compatible with the organization's existing IP-PBX/Call Manager and network infrastructure.
Accessories
Handset, handset cord, stand and all standard accessories.
Warranty
Minimum 1-year OEM warranty; 3 years preferred.
Condition
Brand new, unused and current production model.

	02
	
	

	Multimedia & Online Training Setup

Toll-Free Package

Rack/Tower Server for Database (Data Centre)

	7
	Multimedia & Online Training Setup
· Resolution: 3840 x 2160 (4K UHD)

· Light Source Type: Single Laser

· Light Source Life: 20000hrs

· Throw Ratio: 0.25

· Screen Size: 90~120'

· Projection Distance for 100": 303mm

· Digital Keystone Correction: Yes

· Eye Protection Mode: Yes

· Display Type: DLP

· Brightness (ANSI Lumens): 2200 (Peak)

· Noise: 32dB(A)

· HDR (High Dynamic Range): HDR

· Dolby Digital Plus: Yes

· WiFi
Rack/Tower Server for Database (Data Centre)
Parameter
Minimum Required Specification
System Type
Professional, business/enterprise-class Tower Workstation suitable for continuous operation and server/workstation workloads.
Processor
Workstation-class processor only: Intel Xeon W series / AMD Ryzen Threadripper PRO series or equivalent; minimum 8 physical cores and 16 threads; current generation at the time of bidding.
Memory
Minimum 64 GB ECC DDR5 RAM, expandable to at least 128 GB.
OS / Boot Storage
Minimum 1 TB PCIe NVMe SSD.
Data Storage
2 × 8 TB enterprise-grade drives configured in RAID 1, providing approximately 8 TB usable redundant storage.
RAID
OEM-supported hardware RAID or equivalent, with monitoring and drive-failure notification.
Drive Interface
SATA 6 Gb/s or better.
Storage Expansion
Chassis must support additional internal storage drives.
Graphics
Integrated or entry-level professional graphics sufficient for system administration and standard display requirements.
Network
Minimum 1 × Gigabit Ethernet; 2.5 GbE or higher preferred.
Expansion
PCIe expansion capability for additional network/storage controllers.
Security
TPM 2.0, Secure Boot and BIOS/UEFI password support.
Power Supply
OEM high-efficiency power supply adequately sized for the offered configuration.
Operating System
As required by the purchaser; server operating system licensing may be specified separately.
Accessories
OEM wired keyboard and mouse, all RAID/storage mounting accessories and required cables.
Warranty
Minimum 3-year OEM warranty, preferably on-site.
Condition
Brand new, unused and current production model.

	01
	
	


Lot 02- Procurement and Installation of equipment to establish Digital Agri-Advisory Studio

	
	Peanut Butter Machine (Colloid Mill)

	1
	
Capacity: 10-50kg/hr
 Power: 1.5KW 
Fineness: 2-40μm
Grinding Disc Diameter: 50mm 
Dimensions (mm): 270*500*700
Weight: 60kg
 
	01
	
	
	

	
	Peanut Sheller

	2
	Capacity: 150 kg/hour; 
Shelling Efficiency: ≥98%
 Kernel Breakage: ≤ 5%
Power: 3KW

	01
	
	
	

	
	Peanut Roaster



	3
	Capacity: 8kg/hr Speed: Variable

Power Source: Gas/Electric
	01
	
	
	

	
	Baking Oven (Rotary)

	4
	Tray: 5

Speed: Variable

Power Source: Electric 

Power: 8.2KW

	01
	
	
	

	
	Batter Mixer (Planetary Mixer)



	5
	Capacity: 10L

Speed: Variable 

Power: 0.45KW
	01
	
	
	

	
	High-Speed Vacuum Homogenizer

	6
	Capacity: 5L

Speed: Variable

Emulsifying Motor RPM: 3600

Vacuum Pump: 0.37KW

 Power: 0.55KW
	01
	
	
	


Name: ________________________________________        

Contact Number: ________________________________ 

Office Address: __________________________________

Signature & Stamp: _____________________________  

GENERAL TERMS AND CONDITIONS
Unless the context indicates otherwise, the term “Buyer” refers to PPAF. The term “Supplier” refers to the entity named on the order and contracting with the Buyer. The term “Contract” can be taken to mean either (a) the purchase order or (b) the supply/service agreement, whichever is in place. 

1) Assignment: The Supplier shall not assign, transfer, sublet or subcontract the contract or any part thereof without the prior written consent of the Buyer.

2) Observance of Law: The Supplier shall comply with all laws, ordinances, rules and regulations bearing upon the performance of its obligations under the terms of the contract.

3) Force Majeure: The meaning of the term can be taken to mean acts of God, war (declared or not), invasion, revolution, insurrection or acts similar in nature or force.

3.1) In the event of and as soon as possible after the occurrence of any cause deemed force majeure, the Supplier must inform the Buyer of the full particulars in writing. If the supplier is rendered unable either in part or in whole to perform its obligations then the Buyer shall take such action as it considers, in its sole discretion, to be appropriate or necessary in the circumstances.

3.2) if the Supplier is permanently rendered incapable in whole or part by reason of force majeure to complete its obligations and responsibilities under the contract then the Buyer will have the right to suspend or terminate the contract on the same terms and conditions laid out in section 9, Cancellation.

4) Cancellation: PPAF reserves the right to cancel the contract and /or suspend its activities or through changes to its mandate by virtue of the Management of PPAF. In such a case the Supplier shall be reimbursed by PPAF for completed work/task incurred by the Supplier, including all materials satisfactorily delivered and conforming to specification and terms of contract, prior to receipt of the termination notice.

4.1) Should the supplier encounter solvency problems including, but not limited to, bankruptcy, liquidation, receivership and similar, the PPAF reserves the right to terminate the contract immediately without prejudice to any other right or remedy it may have under the terms of these conditions.

5) Inspection and Test: The Supplier must inspect the goods prior to dispatch to ensure conformance to specification and/or any other provisions of the contract. The PPAF reserves the right to inspect the goods for compliance with specifications and provisions of the contract. If, in PPAFs’ opinion, the goods and/or services do not comply with the specification, the PPAF will inform the Supplier in writing. In such a case the Supplier shall take the necessary action to ensure compliance, liability for any additional cost incurred for rectifying compliance will rest with the Supplier.

6) Changes: The PPAF reserves the right to make reasonable changes at any time to the specification, quantity, destination, or delivery instruction. If any such change affects the price of goods or performance of service the Supplier and PPAF may negotiate an equitable adjustment to the contract, provided that the Supplier claims for adjustments in writing to the PPAF within the contractual period from being notified of any change.

7) Payment Terms: Unless otherwise agreed, payment shall be made upon submission of invoice within 15 working days, subject to satisfactory completion of the assignment (upon verification by PPAF). 
8) Environmental Standards - Suppliers should as a minimum, comply with all statutory and other legal requirements relating to environmental impacts of their business. Areas which should be considered are:

· Waste Management
· Packaging and Paper 

· Conservation 

· Energy Use 

· Sustainability 

09) Anti-Money Laundering and Anti-Terrorism Financing Policy

“It is the policy of the PPAF to prohibit and actively prevent money laundering and any activity that facilitates money laundering or the funding of terrorism or criminal activities” by complying with all applicable requirements under the Anti-Money Laundering Act 2010 (Act No. VII of 2010 - an Act to provide for prevention of money laundering) and Anti-Terrorism (Second Amendment) Act, 2014 and its implementation regulations. Recently under the national action plan and SECP regulations money laundering has been identified as a major cause for corruption and criminal activities. 
4

